Agenda for the PPP Working Group¥The PPP Banyan Vines Control Protocol (BVCP)— draft-ietf-pppext-vines-01.txt¥The PPP XNS IDP Control Protocol (XNSCP)— draft-ietf-pppext-xnscp-00.txt¥The PPP Encryption Control Protocol (ECP)— draft-ietf-pppext-encryption-00.txt¥PPP for Data Compression in Data Circuit-Terminating Equipment (DCE)— draft-ietf-pppext-dce-compress-00.txt¥PPP LZS-DCP Compression Protocol (LZS-DCP)— draft-ietf-pppext-lzs-dcp-00.txt¥PPP Serial Data Transport Protocol (SDTP)— draft-ietf-pppext-sdtp-00.txtThe PPP Banyan Vines Control Protocol (BVCP)¥This document defines the Network Control Protocol for establishing and configuring the Banyan VINES protocol over PPP.BVCP Configuration Options Value Option 1 BV-NS-RTP-Link-Type 2 BV-FRP 3 BV-RTPBV-NS-RTP-Link-Type¥... provides a way to negotiate the way the 4.11 Non-Sequenced Routing Update Protocol (NS-RTP) will run on the link.¥The acceptance of this option (by the peer) indicates that the peer will send NS-RTP updates as if the link was a LAN type. ¥The rejection (or absence) of this option indicates that the peer will send NS-RTP updates as if the link was a WAN type.— 0 1— 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5— +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+— | Type | Length |— +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+BV-FRP¥This Configuration Option provides a way to negotiate the use of VINES Fragmentation Protocol (FRP). ¥If an MRU of less than 1484 is negotiated, FRP will be needed to send a full size VINES packet over the link.— 0 1— 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5— +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+— | Type | Length |— +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+BV-RTP¥This Configuration Option provides a way to negotiate whether RTP is used over the link. ¥If dial-up lines with static routes are being used, the use of RTP may be totally suppressed to conserve bandwidth on the link.¥By default, RTP packets are sent over the link.— 0 1— 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5— +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+— | Type | Length |— +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

The PPP XNS IDP Control Protocol (XNSCP)¥This document defines the Network Control Protocol for establishing and configuring the Xerox Network Systems (XNS) Internet Datagram Protocol (IDP) over PPP.¥XNSCP has no Configuration Options.