cisco Systems

IGMP RP-Report Message • New host message to advertise Rendezvous Point (RP) addresses for multicast groups • Any system may send an RP-Report even if it is not a member of the group • Much like Host-Reports:

Sent when Host-Query is received Suppressed when others respond first • Sender can request shared RP-tree or source SPT-tree • Requirements:

All RP reporters must include all RPs for a group RP list must be consistent amoung reporters

cisco Systems

Packet Format