Session Advertisement via WWW

ffl WWW’s HTTP 1.0 uses MIME to deliver documents

ffl Create an experimental application-specific MIME type, application/x-sd

ffl Specify my sd-launch program as the program to interpret application/x-sd files

n=2261714691 2261714691 764620273
s=Sample Session
i=This is a sample session for a slide for my\
 confctrl presentation
o=fenner@herman.cmf.nrl.navy.mil
c=224.2.189.49 16 2850600496 2850607696
m=audio 49077 33755
m=video 61697 20598
m=whiteboard 40170 22538

Modifications necessary

ffl Clients require simple modification to ~ /.mailcap file ffl Extensions to Plexus 3.0 server, and the sd-listen program posted to rem-conf, to implement server side ffl This experimental server is at

http://herman.cmf.nrl.navy.mil:8001/sd/

ffl Any server supporting returning arbitrary file types can return sessions in response to queries

Media on Demand via WWW

ffl Anders Klemets wrote the server extensions, scripts are available ffl Server is at http://www.it.kth.se/~ klemets/vatplay.html ffl Can provide both previously recorded sessions (using ’ vat record’ or ’nv record’), or .au (or .au.gsm) files ffl Unicast only, multicast on demand is somewhat more dangerous and it’s harder to decide when to stop transmitting