cisco IP Multicast Release Status

Dino Farinacci cisco Systems dino@cisco.com

IETF Mbone BOF December 4, 1995

c i s c o S y s t e m s

Agenda

• Release 10.2 and 10.3 • Release 11.0 • Miscellaneous Features • Release 11.1 and Future

c i s c o S y s t e m s

Release 10.2 and 10.3

• 10.2 shipped in October ‘94 Contains Sparse- and Dense-mode PIM version 1 Limited DVMRP interoperability support DVMRP and GRE tunnels mrinfo support Multicast related MIB support • 10.3 shipped in March ’95 10.2 and 10.3 are multicast feature compatible Bug fixes track each other • General Availability

10.2(10) 10.3(7)

c i s c o S y s t e m s

Release 11.0

• New feature release shipped in September ‘95 Current release is 11.0(3.3) *** Don’t use my images *** • Fastswitching support - including tunnels • DVMRP Pruning/Grafting

Mapped into and out of PIM Prunes/Grafts/Joins • mtrace responder and command support • mrinfo command support • Rate limiting and Weighted Fair Queuing • sd listener support

c i s c o S y s t e m s

DVMRP Unicast Routing

• Put into 10.2, 10.3, and 11.0 • The current way to do policy based multicast Unicasts go one way, Multicasts go another • ciscos run Sparse-mode PIM over MBONE topology using DVMRP routes to RPF Allows a transit PIM region between DVMRP regions ISPs run PIM, they connect their clients to the MBONE using PIM or DVMRP

c i s c o S y s t e m s

Miscellaneous Stuff

• DVMRP Default Routing

In all releases Will originate/propagate default route • DVMRP Route Summarization

By default, ciscos send classful routes into MBONE Can send CIDR routes • Reporting facility to track MBONE route surges

•  show ip mroute active

c i s c o S y s t e m s

Release 11.1 - now beta testing

• Scoped Address support • IGMP v2 • PIM SPT switching thresholds

Futur e

• PIM v2

Send Questions/Comments/Bug Reports

• multicast-support@cisco.com