Support for Mobile NHRP

Devices

NEC & CiTR

Auto Configuration of NHRP

Clients

Hiroshi Suzuki NEC David Horton

CiTR

�Painful� Task

¥Configuration of large number of Clients

—Physical topology changes:

¥Clients Move & # Increases/Decreases

¥Servers Move/Disappear

—Logical topology changes

¥LIS membership changes

¥New LISs are generated

—LIS is very dynamic

Configuration

Auto Configuration of NHRP

Clients

¥When we need it ?

—When NHS ( NHRP Server ) moves

—When NHC ( NHRP Client ) moves

—When LIS member ship changes

—(Always if NHRP supports more than one LIS)

¥Why not Configuration Server ?

—Configuration server needs �Configuration� for all the

above cases