Page 1129_025/c51

Trunk MIB Working GroupFred BakerCisco Systems129_025/c52

dsx1Fdl¥Issue: - the comment says it is a bit vector but the SYNTAX is an enumerated type¥Solution? - deprecate (obsolete ?) the existing object and create a new one with the correct SYNTAX - see dsx1LineStatus for an example. Note that it is in fact possible to run both T1.403 and PUB 54016 msgs on the FDL at the same time (the address bytes have distinct values) so we do need the bit bector.129_025/c53

dsx1LineIndex/dsx1IfIndex¥Issue: - in the absence of RFC 1573 we need to allow for T1 lines without interfaces. ¥Solution? - Declare we only support the "External Interface Scenario" in Section 3.1129_025/c54

the dreaded fractional table - is it needed ? ¥Issue: - Given an ifEntry that represents the DS0 bundle do we need the frac Table at all or should the DS0s that comprise the bundle be identified in attributes of the bundles ifEntry instead of in the frac table entry for the DS1 ?¥Solution? - For "raw bits" (case (a) above) I don’t think you need to move the information. For the BONDING case where you are BONDING across multiple interface you need info in the BONDING interface but that is probably a different ifType than the "raw bits" case. If we keep the frac table it gives us somewhere to put the per-circuit signalling controls...129_025/c56

Loopbacks¥Issue: - the current loopback control variable only allows you to apply outward directed loopbacks. Inward-directed loopbacks are useful too.¥Solution? - Add new values to the enumeration and hope our advisor doesn’t tell us we have to use the test table instead

Page 2129_025/c57

UAS Fixup¥Issue: - Despite a direct note in the text, folks still ask about the UAS fixup - go back and adjust things +/- 10. ¥Solution? - Make the note brutally direct and clear 129_025/c58

dsx1SendCode¥Issue: - From time to time someone asks whether this object is meant to be a "knob" or an "LED".¥Solution? - Clarify that is is a knob.129_025/c59

Per-Circuit Configuration¥Issue: - There isn’t any in the MIB. At least one set of folk asked for it last fall (Sprint) and Newbridge could use it. ¥Solution? - Consider adding an object, perhaps in the dreaded frac table, to say whether a given timeslot has bit-oriented signalling on or off. This is probably T1 only given that CAS mode in E1 doesn’t rob from a channel... 129_025/c510

References to T1M1.3/92-005R1.¥Issue: - ANSI finally issued the real document - it is T1.231 ¥Solution? - Update all references129_025/c512

Some Performance Parameters Don’t Have References ¥Issue: - Some of the performance parameter definitions (e.g. CSS) provide a definition without a reference. This leads to the odd person questioning/suggestesting other answers, etc.¥Solution? - Ensure each performance parameter has a reference in the text of the definition. Whether or not we put them in the REFERENCE clause for each object is a good question.

Page 3129_025/c513

Row Creation¥Issue: - There is no way for a management station to create a row in the dsx1ConfigTable. One could argue that T1s are physical things and thus the agent should be the one to populate the dsx1ConfigTable not the NMS. ¥Solution? - Make the foregoing argument explicitly in the document add an object with type RowStatus to the config table. 129_025/c514

dsx1LineType¥Issue: - There is not line type for transparent lines with no framing ¥Solution? - Add a new line type129_025/c515

SNMPv2¥Issue: - All MIBs must be submitted in SNMPv2 syntax ¥Solution - Just do it129_025/c516

DS2 Support¥Issue: - DS2s are not supported by either MIB. ¥Solution? - Use the DS1 MIB to support DS2. This requires the addition of a few objects and some textual changes. A proposal was submitted to the list by Yasuhiko Hato.