Page 1517_075/c11

Integrated Services MibFred BakerCisco Systems517_075/c12

Intent Of Mib¥Display Protocol Independent Information¥Display Sessions Active¥Configure/Display Interface Characteristics¥Protocol Dependent Information Left To RSVP/ST-II Mibs517_075/c13

Textual Conventions¥IP Protocol¥UDP/TCP Port¥Bit Rate517_075/c14

Interface Attributes¥Index Interface Index (ifIndex)¥ConfiguresMaximum Bit Rate ReservableMaximum Bit Rate Reservable By One Stream¥DisplaysCurrent Allocated Bit RateAdd Current Delay Experienced?