Page 1517_075/c11

RSVP Management Information BaseFred BakerCisco Systems517_075/c12

Textual Conventions¥RSVP Encapsulation¥Refresh Interval¥QoS Service¥Delay Class¥Burst Size¥Time To Live (TTL)¥IP Address String517_075/c13

Tables¥Session Senders¥Session Reservations¥Session Reservation Requests¥Interface Attributes517_075/c14

Session Sender Database Attributes¥Time To Live (TTL)¥Sender TSpec Token Bucket¥Previous Hop Interface, Address¥Refresh Interval¥Time Of Last Change517_075/c16

Session Reservation Database¥List Of RESV Messages Received¥IndexDestination Address, Protocol, PortSource Address, PortNext Hop Interface, Address

Page 2517_075/c17

Session Reservation Database Attributes¥RSpecToken BucketDelay ClassRequested QoS Service¥Refresh Interval¥Scope (List Of IP Addresses)¥Is Reservation Shared/Distinct?¥Is Reservation Explicit/Wildcard?¥Time Of Last Change517_075/c18

Session Reservation Request Database¥List Of RESV Messages Being Sent¥IndexDestination Address, Protocol, PortSource Address, PortPrevious Hop Interface, Address517_075/c19

Session Reservation Request Database Attributes¥RSpecToken BucketDelay ClassRequested QoS Service¥Refresh Interval¥Scope (List Of IP Addresses)¥Is Reservation Shared/Distinct?¥Is Reservation Explicit/Wildcard?¥Time Of Last Change517_075/c110